Basin: Development Template
     Description: Bulletin 75 Rainfall Data
     Last Modified Date: 22 May 2020
     Last Modified Time: 20:00:59
     Version: 4.3
     Filepath Separator: \
     Unit System: English
     Missing Flow To Zero: No
     Enable Flow Ratio: No
     Compute Local Flow At Junctions: No

     Enable Sediment Routing: No

     Enable Quality Routing: No
End:

Subbasin: Detained Area
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:51:58
     Canvas X: -372.71679152110903
     Canvas Y: 1441.3583081779193
     Label X: -3.0
     Label Y: 4.0
     Area: 0.00625
     Downstream: Detention Facility

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: SCS
     Percent Impervious Area: 0.0
     Curve Number: 89.15

     Transform: SCS
     Lag: 6
     Unitgraph Type: STANDARD

     Baseflow: None
End:

Reservoir: Detention Facility
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:51:50
     Canvas X: -372.71679152110903
     Canvas Y: 1337.566467771835
     Label X: -1.0
     Label Y: 4.0
     Downstream: Gross Release Rate

     Route: Modified Puls
     Routing Curve: Storage-Elevation-Outflow
     Initial Outflow: 0
     Storage-Outflow Table: Detention Facility
     Elevation-Storage Table: Detention Facility
     Primary Table: Storage-Outflow
End:

Subbasin: Unrestricted Area
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:57:08
     Canvas X: -159.49695015799472
     Canvas Y: 1332.364343158686
     Label X: -2.0
     Label Y: 2.0
     Area: .00078125
     Downstream: Gross Release Rate

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: SCS
     Percent Impervious Area: 0.0
     Curve Number: 80

     Transform: SCS
     Lag: 6
     Unitgraph Type: STANDARD

     Baseflow: None
End:

Subbasin: Development
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:57:26
     Canvas X: 91.5067089866422
     Canvas Y: 1344.191740710004
     From Canvas X: -336.84991126091506
     From Canvas Y: 73.83011753663868
     Label X: -4.0
     Label Y: 4.0
     Area: 0.00625
     Downstream: Overflow Weir

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: SCS
     Percent Impervious Area: 0.0
     Curve Number: 95.28

     Transform: SCS
     Lag: 6
     Unitgraph Type: STANDARD

     Baseflow: None
End:

Subbasin: Upstream Tributary
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:57:51
     Canvas X: 312.28479661124425
     Canvas Y: 1341.5634301430443
     From Canvas X: -908.637159012211
     From Canvas Y: -1096.2789843811456
     Label X: -2.0
     Label Y: 5.0
     Area: 0.001875
     Downstream: Overflow Weir

     Canopy: None
     Allow Simultaneous Precip Et: No
     Plant Uptake Method: None

     Surface: None

     LossRate: SCS
     Percent Impervious Area: 0.0
     Curve Number: 83

     Transform: SCS
     Lag: 6
     Unitgraph Type: STANDARD

     Baseflow: None
End:

Junction: Overflow Weir
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:54:24
     Canvas X: 203.17419676125547
     Canvas Y: 1232.3689548670498
     From Canvas X: 737.0889966921873
     From Canvas Y: 957.3419296329738
     Label X: -46.0
     Label Y: -27.0
End:

Junction: Gross Release Rate
     Last Modified Date: 20 May 2020
     Last Modified Time: 17:51:10
     Canvas X: -263.46222267259935
     Canvas Y: 1228.3118989233253
     From Canvas X: -346.70968916455763
     From Canvas Y: 838.6383159475531
     Label X: -60.0
     Label Y: -27.0
End:

Basin Layer Properties:
     Element Layer:
          Name: Icons
          Layer shown: Yes
     End Layer:
End:

Basin Spatial Properties:
End:

Basin Schematic Properties:
     Last View N: 3008.213552361396
     Last View S: -1236.2013938703703
     Last View W: -2002.0533880903495
     Last View E: 1201.23203285421
     Maximum View N: 1352.645536407811
     Maximum View S: 0.0
     Maximum View W: -532.6042050702517
     Maximum View E: 571.7872477512959
     Extent Method: Elements
     Buffer: 0
     Draw Icons: Yes
     Draw Icon Labels: Name
     Draw Map Objects: No
     Draw Gridlines: No
     Draw Flow Direction: No
     Draw HillShade Layer: Yes
     Draw Elevation Layer: Yes
     Elevation Layer Color Palette: Default
     Ignore Elevation Color Ramp Scale: No
     Use Interpolated Color Ramp for Elevation Layer: Yes
     Color Ramp Opacity Level for Elevation Layer: 33.0
     Fix Element Locations: No
     Fix Hydrologic Order: No
End:
